Usage:

Connect to the “WiFi” of the router you want to use

As of writing this, the password should be the same as the name

Write the Router’s IP address into the IP textbox

Hit the scan button

Connect to each patch before pairing to it

The list of patches to connect updates every time a patch is found

but only updates alphabetically every time the connect window is opened, same with the pair window

Hit start streaming even if just using one patch. Do not hit it twice.

Hit stop streaming to stop the sampling for all patches

Make sure to hit Export before hitting Disconnect all

THE DISCONNECT ALL BUTTON EMPTYS ALL OF THE DATA GATHERS THUS FAR